
CCNA Lab Topology Arizona



Objective

1. Deploy a base configuration for all devices including
   1. Hostname
      * Enable
      * Configure terminal
      * Hostname “name”
   2. Logon banner
      * Enable
      * Configure terminal
      * Banner motd line
   3. Synchronous logging
      * Enable
      * Configure terminal
      * Line console 0
      * Logging synchronous
        1. Keeps the status messages out of the way
   4. Console passwords
      * Enable
      * Configure terminal
      * Line console 0
      * Password “cisco”
      * Login (make it require the password)
   5. Telnet passwords
      * Enable
      * Configure terminal
      * Line vty 0 4
      * Login
      * Password “cisco”
   6. Protect privilege mode
      * enable
      * configure terminal
      * enable secret cisco
   7. Ip addressing
      * 192.168.1.0/24 for now
   8. Activating interfaces
      * Show ip interface brief
      * Enable
      * Configure terminal
      * Int g0/0 192.168.1.1 255.255.255.0
   9. No domain lookups
      * Enable
      * Configure terminal
      * No ip domain-lookup
   10. Password encryption service3
       * Enable
       * Configure terminal
       * Service password-encryption
   11. Save configuration
       * Enable
       * Wr
         1. OR YOU CAN WRITE THE ENTIRE COMMAND
       * Copy running-config startup-config